SCG Engineering Release Notice
Phase12 GCA Release Version 12.00.00.00 - SAS2FLASH_Phase12.0 (SCGCQ00228725)


Phase12 GCA Release Version 12.00.00.00 - SAS2FLASH_Phase12.0 (SCGCQ00228725)
Defects=0, Enhancements=0 (Version Change Only)

Phase12 Beta Release Version 11.250.03.00 - SAS2FLASH_Phase12.0 (SCGCQ00227559)
Change Summary ( Defects=1)
SCGCQ00227229 (DFCT) - SAS2FLASH validation fails when downloading firmware on a Mustang with Device Id 0x6E


Phase12 Beta Release Version 11.250.02.00 - SAS2FLASH_Phase12.0 (SCGCQ00225278)
Change Summary ( Defects=3)
SCGCQ00201406 (DFCT) - SAS2FLASH does not properly handle flashing IR firmware for TBOLT & Mustang cards when no NVSRAM is Present
SCGCQ00220979 (DFCT) - Sas2flash: Sas2flash.EFI -e 7 erase options fails for Thunderbolt B0.
SCGCQ00223355 (DFCT) - SAS2FLASH: Seg Fault occurs on giving a non existing controller index in sas2flash

Phase12 Alpha Release Version 11.250.01.00 - SAS2FLASH_Phase12.0 (SCGCQ00218922)
Change Summary ( Enhancements=4)
SCGCQ00193200 (ENHREQ) - SAS2FLASH: Support multiple NVDATA images in FW image to support flashing TBolt D0
SCGCQ00195753 (ENHREQ) - Add support for Tbolt/Mustang C1 and D0 chip revisions
SCGCQ00198463 (ENHREQ) - Sas2Flash: Add an option to not issue adapter reset on a firmware download
SCGCQ00208316 (ENHREQ) - SAS2Flash display of FW fault code




