SCG Engineering Release Notice
Phase12 GCA Release Version 7.23.01.00 - SAS2BIOS_Phase12.0 (SCGCQ00229883)
Change Summary ( Defects=1)
SCGCQ00229773 (DFCT) - With IT firmware BIOS CU throws CONFIG PAGE ERROR: 0x0A80822


Phase12 Beta Release Version 7.22.03.00 - SAS2BIOS_Phase12.0 (SCGCQ00227519)
Change Summary ( Defects=1)
SCGCQ00220990 (DFCT) - BIOS CU freezes for 4 minutes after removing a volume from the controller.

Phase12 Beta Release Version 7.22.02.00 - SAS2BIOS_Phase12.0 (SCGCQ00225222)
Change Summary ( Defects=3)
SCGCQ00220215 (DFCT) - Help text screen for "Drive Status" is over writing footer line.
SCGCQ00220966 (DFCT) - "SAS Address NOT Programmed on controller in slot " message gets displayed twice in BIOS Banner
SCGCQ00221758 (DFCT) - Direct attached drives connected to an IT controller not discovered after issuing refresh in BIOS.


Phase12 Alpha Release Version 7.22.01.00 - SAS2BIOS_Phase12.0 (SCGCQ00219516)
Change Summary ( Enhancements=3)
SCGCQ00189177 (ENHREQ) - Enhance Legacy BIOS CU to refresh status reflecting IR RAID Volume member disks during Sync
SCGCQ00197065 (ENHREQ) - Implement PI filtering for IR volume creation in BIOS CU.
SCGCQ00197342 (ENHREQ) - Display the "Device Identifier" in SAS topology with space separation between "Vendor" and "Product" identifications.














